[bookmark: _GoBack]X-Long End Jaw Specs. Jaw width: 3". Jaw capacity: 3". Shaft length: 8". Weight: 21 oz.
All Cardellini Clamps Feature: Rust-proof construction: stainless steel shaft and bushing, aluminum jaws and knob. Patented Jaw design firmly grips almost any shape. Quick spin knobs reduce setting and release times. Jaw pads grip and protect the surface being clamped, and are easily replaceable in case of damage. Heavy threads on the shaft resist dinging.
